<?xml version="1.0" encoding="UNICODE" ?>
<topo version="1.2.00.510">
    <devices>
        <dev id="E7A6FE6B-B67F-44b1-B7D0-14C07108BEE0" name="PC2" poe="0" model="PC" settings=" -simpc_ip 192.168.20.2  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.20.1  -simpc_mac 54-89-98-CE-3A-BF  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-CE-3A-BF" com_port="0" bootmode="0" cx="392.000000" cy="406.000000" edit_left="419" edit_top="460">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="0F164522-C4E4-4490-81B6-09909E1C0977" name="PC3" poe="0" model="PC" settings=" -simpc_ip 172.16.1.2  -simpc_mask 255.255.255.0  -simpc_gateway 172.16.1.1  -simpc_mac 54-89-98-D1-57-32  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-D1-57-32" com_port="0" bootmode="0" cx="492.000000" cy="127.000000" edit_left="519" edit_top="181">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="3709B0C9-3E06-49fe-B8B4-40CFDB23CB73" name="LSW1" poe="0" model="S5700" settings="" system_mac="4C-1F-CC-0C-7B-CF" com_port="2001" bootmode="0" cx="307.000000" cy="257.000000" edit_left="334" edit_top="311">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="24" />
            </slot>
        </dev>
        <dev id="8EF3E09C-CE82-4580-8059-237CA2013843" name="FW1" poe="0" model="USG6000V" settings="" system_mac="00-E0-FC-E3-51-F3" com_port="2000" bootmode="0" cx="305.000000" cy="132.000000" edit_left="332" edit_top="186">
            <slot id="1">
                <interface category="Ethernet" type="GE" slotIndex="0" cardIndex="0" interfaceIndex="0" />
                <interface category="Ethernet" type="GE" slotIndex="1" cardIndex="0" interfaceIndex="0" />
                <interface category="Ethernet" type="GE" slotIndex="1" cardIndex="0" interfaceIndex="1" />
                <interface category="Ethernet" type="GE" slotIndex="1" cardIndex="0" interfaceIndex="2" />
                <interface category="Ethernet" type="GE" slotIndex="1" cardIndex="0" interfaceIndex="3" />
                <interface category="Ethernet" type="GE" slotIndex="1" cardIndex="0" interfaceIndex="4" />
                <interface category="Ethernet" type="GE" slotIndex="1" cardIndex="0" interfaceIndex="5" />
                <interface category="Ethernet" type="GE" slotIndex="1" cardIndex="0" interfaceIndex="6" />
            </slot>
        </dev>
        <dev id="DA44F485-3BCD-493e-88BD-5F92C1F83552" name="PC1" poe="0" model="PC" settings=" -simpc_ip 192.168.10.2  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.10.1  -simpc_mac 54-89-98-73-79-7D  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-73-79-7D" com_port="0" bootmode="0" cx="215.000000" cy="409.000000" edit_left="242" edit_top="463">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
    </devices>
    <lines>
        <line srcDeviceID="8EF3E09C-CE82-4580-8059-237CA2013843" destDeviceID="3709B0C9-3E06-49fe-B8B4-40CFDB23CB73">
            <interfacePair lineName="Copper" srcIndex="1" srcBoundRectIsMoved="0" srcBoundRect_X="332.690857" srcBoundRect_Y="202.178238" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="333.309143" tarBoundRect_Y="240.821762" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="3709B0C9-3E06-49fe-B8B4-40CFDB23CB73" destDeviceID="DA44F485-3BCD-493e-88BD-5F92C1F83552">
            <interfacePair lineName="Copper" srcIndex="1" srcBoundRectIsMoved="0" srcBoundRect_X="311.639343" srcBoundRect_Y="320.943726" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="264.360657" tarBoundRect_Y="399.056274" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="3709B0C9-3E06-49fe-B8B4-40CFDB23CB73" destDeviceID="E7A6FE6B-B67F-44b1-B7D0-14C07108BEE0">
            <interfacePair lineName="Copper" srcIndex="2" srcBoundRectIsMoved="0" srcBoundRect_X="355.398041" srcBoundRect_Y="321.509491" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="397.601959" tarBoundRect_Y="395.490509" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="8EF3E09C-CE82-4580-8059-237CA2013843" destDeviceID="0F164522-C4E4-4490-81B6-09909E1C0977">
            <interfacePair lineName="Copper" srcIndex="2" srcBoundRectIsMoved="0" srcBoundRect_X="375.168335" srcBoundRect_Y="157.845764" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="475.831665" tarBoundRect_Y="155.154236" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
    </lines>
    <shapes />
    <txttips>
        <txttip left="205" top="491" right="300" bottom="508" content="192.168.10.2" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="401" top="493" right="496" bottom="510" content="192.168.20.2" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="533" top="90" right="612" bottom="107" content="172.16.1.2" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
    </txttips>
</topo>
