<?xml version="1.0" encoding="UNICODE" ?>
<topo version="1.2.00.510">
    <devices>
        <dev id="C4E2B52C-EB07-42b8-9D39-9BCE785474E2" name="AR1" poe="0" model="AR1220" settings="" system_mac="00-E0-FC-FB-5D-61" com_port="2000" bootmode="0" cx="370.000000" cy="77.000000" edit_left="397" edit_top="131">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="2" />
                <interface sztype="Ethernet" interfacename="Ethernet" count="8" />
            </slot>
        </dev>
        <dev id="BBA2D23B-6680-4979-B05B-1638B97BEECB" name="PC1" poe="0" model="PC" settings=" -simpc_ip 192.168.10.253  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.10.254  -simpc_mac 54-89-98-1F-38-25  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 192.168.1.1  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 1  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 1  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-1F-38-25" com_port="0" bootmode="0" cx="279.000000" cy="384.000000" edit_left="306" edit_top="438">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="D6AEFE97-08BF-440a-B8CC-ECF4046C9938" name="PC2" poe="0" model="PC" settings=" -simpc_ip 192.168.20.253  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.20.254  -simpc_mac 54-89-98-55-61-C4  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 192.168.1.1  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 1  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 1  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-55-61-C4" com_port="0" bootmode="0" cx="491.000000" cy="384.000000" edit_left="518" edit_top="438">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="983721F6-FFE4-4471-9EDC-C626EF1ABBA5" name="LSW1" poe="0" model="S5700" settings="" system_mac="4C-1F-CC-2E-7B-4F" com_port="2001" bootmode="0" cx="370.000000" cy="216.000000" edit_left="397" edit_top="270">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="24" />
            </slot>
        </dev>
    </devices>
    <lines>
        <line srcDeviceID="C4E2B52C-EB07-42b8-9D39-9BCE785474E2" destDeviceID="983721F6-FFE4-4471-9EDC-C626EF1ABBA5">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="397.000000" srcBoundRect_Y="147.183762" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="397.000000" tarBoundRect_Y="199.816238" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="983721F6-FFE4-4471-9EDC-C626EF1ABBA5" destDeviceID="BBA2D23B-6680-4979-B05B-1638B97BEECB">
            <interfacePair lineName="Copper" srcIndex="1" srcBoundRectIsMoved="0" srcBoundRect_X="376.432312" srcBoundRect_Y="280.971130" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="326.567688" tarBoundRect_Y="373.028870" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="983721F6-FFE4-4471-9EDC-C626EF1ABBA5" destDeviceID="D6AEFE97-08BF-440a-B8CC-ECF4046C9938">
            <interfacePair lineName="Copper" srcIndex="2" srcBoundRectIsMoved="0" srcBoundRect_X="422.237976" srcBoundRect_Y="278.041138" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="492.762024" tarBoundRect_Y="375.958862" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
    </lines>
    <shapes />
    <txttips>
        <txttip left="451" top="130" right="576" bottom="147" content="192.168.2.254/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="263" top="326" right="312" bottom="343" content="vlan10" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="487" top="327" right="536" bottom="344" content="vlan20" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
    </txttips>
</topo>
