<?xml version="1.0" encoding="UNICODE" ?>
<topo version="1.2.00.510">
    <devices>
        <dev id="524E18C9-E11B-4b3c-8897-3398E5AE6F08" name="LSW1" poe="0" model="S5700" settings="" system_mac="4C-1F-CC-3A-3C-B2" com_port="2000" bootmode="0" cx="201.000000" cy="408.000000" edit_left="228" edit_top="462">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="24" />
            </slot>
        </dev>
        <dev id="87B7FA53-8EFD-4733-8D6C-CF612AA68C72" name="AR2" poe="0" model="AR1220" settings="" system_mac="00-E0-FC-19-45-D1" com_port="2002" bootmode="0" cx="419.000000" cy="211.000000" edit_left="446" edit_top="265">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="2" />
                <interface sztype="Ethernet" interfacename="Ethernet" count="8" />
            </slot>
        </dev>
        <dev id="F4C19C55-2E1C-48f9-A31B-152EAAA9889C" name="PC2" poe="0" model="PC" settings=" -simpc_ip 192.168.20.2  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.20.254  -simpc_mac 54-89-98-98-13-45  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-98-13-45" com_port="0" bootmode="0" cx="291.000000" cy="586.000000" edit_left="318" edit_top="640">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="1E3F0372-B565-4168-A6E6-9E4D1412CD04" name="PC1" poe="0" model="PC" settings=" -simpc_ip 192.168.10.2  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.10.254  -simpc_mac 54-89-98-E9-24-EB  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-E9-24-EB" com_port="0" bootmode="0" cx="110.000000" cy="586.000000" edit_left="137" edit_top="640">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="825C0D0C-86F8-4981-B7A3-B74E08B8E5F8" name="Server2" poe="0" model="Server" settings="-domain 0 -eth 54-89-98-D3-80-5D -ipaddr 192.168.30.250 -ipmask 255.255.255.0 -gateway 192.168.30.254 -ipv6addr 2000::2 -ipv6gateway 2000::1 -prefixlen 64 -ipv4dns 0.0.0.0 -ipv6dns 3000::1 -dnslist NULL" system_mac="54-89-98-D3-80-5D" com_port="0" bootmode="0" cx="443.000000" cy="412.000000" edit_left="470" edit_top="466">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="5F897AAE-9F5E-480b-985B-9AB2893ABE9D" name="AR1" poe="0" model="AR1220" settings="" system_mac="00-E0-FC-0B-36-F0" com_port="2001" bootmode="0" cx="205.000000" cy="213.000000" edit_left="232" edit_top="267">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="2" />
                <interface sztype="Ethernet" interfacename="Ethernet" count="8" />
            </slot>
        </dev>
        <dev id="3988008A-554A-41a4-9DB2-FA5195A1150E" name="Client1" poe="0" model="Client" settings="-domain 0 -eth 54-89-98-75-09-F9 -ipaddr 202.1.1.2 -ipmask 255.255.255.0 -gateway 202.1.1.254 -ipv6addr 2000::2 -ipv6gateway 2000::1 -prefixlen 64 -ipv4dns 0.0.0.0 -ipv6dns 3000::1 -dnslist NULL" system_mac="54-89-98-75-09-F9" com_port="0" bootmode="0" cx="610.000000" cy="212.000000" edit_left="637" edit_top="266">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
    </devices>
    <lines>
        <line srcDeviceID="1E3F0372-B565-4168-A6E6-9E4D1412CD04" destDeviceID="524E18C9-E11B-4b3c-8897-3398E5AE6F08">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="156.657211" srcBoundRect_Y="574.549622" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="208.342789" tarBoundRect_Y="473.450378" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="F4C19C55-2E1C-48f9-A31B-152EAAA9889C" destDeviceID="524E18C9-E11B-4b3c-8897-3398E5AE6F08">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="298.514618" srcBoundRect_Y="574.462280" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="9" tarBoundRectIsMoved="0" tarBoundRect_X="247.485382" tarBoundRect_Y="473.537750" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="524E18C9-E11B-4b3c-8897-3398E5AE6F08" destDeviceID="5F897AAE-9F5E-480b-985B-9AB2893ABE9D">
            <interfacePair lineName="Copper" srcIndex="23" srcBoundRectIsMoved="0" srcBoundRect_X="228.885635" srcBoundRect_Y="391.825317" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="231.114365" tarBoundRect_Y="283.174683" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="5F897AAE-9F5E-480b-985B-9AB2893ABE9D" destDeviceID="87B7FA53-8EFD-4733-8D6C-CF612AA68C72">
            <interfacePair lineName="Copper" srcIndex="1" srcBoundRectIsMoved="0" srcBoundRect_X="275.181885" srcBoundRect_Y="239.596436" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="1" tarBoundRectIsMoved="0" tarBoundRect_X="402.818115" tarBoundRect_Y="238.403564" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="87B7FA53-8EFD-4733-8D6C-CF612AA68C72" destDeviceID="3988008A-554A-41a4-9DB2-FA5195A1150E">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="489.183167" srcBoundRect_Y="238.226089" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="593.816833" tarBoundRect_Y="238.773911" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="524E18C9-E11B-4b3c-8897-3398E5AE6F08" destDeviceID="825C0D0C-86F8-4981-B7A3-B74E08B8E5F8">
            <interfacePair lineName="Copper" srcIndex="22" srcBoundRectIsMoved="0" srcBoundRect_X="271.177856" srcBoundRect_Y="435.713684" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="426.822144" tarBoundRect_Y="438.286316" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
    </lines>
    <shapes />
    <txttips>
        <txttip left="109" top="675" right="226" bottom="707" content="vlan 10&#x0D;&#x0A;192.168.10.2/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="308" top="672" right="425" bottom="704" content="vlan 20&#x0D;&#x0A;192.168.20.2/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="19" top="360" right="204" bottom="408" content="vlan10:192.168.10.254/24&#x0D;&#x0A;vlan20:192.168.20.254/24&#x0D;&#x0A;vlan30:192.168.30.254/30" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="72" top="279" right="204" bottom="296" content="192.168.30.253/28" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="254" top="183" right="349" bottom="200" content="200.1.1.1/28" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="334" top="258" right="429" bottom="275" content="200.1.1.2/28" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="482" top="203" right="592" bottom="220" content="202.1.1.254/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="601" top="300" right="696" bottom="317" content="202.1.1.2/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="72" top="213" right="167" bottom="245" content="企业ISP接入&#x0D;&#x0A;配置 NAT-PAT" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="786" top="190" right="1228" bottom="316" content="配置过程&#x0D;&#x0A;1、确保R1到达内网的路由，到达外网的路由&#x0D;&#x0A;&#x0D;&#x0A;   ip route-static 192.168.0.0 255.255.0.0 192.168.30.254&#x0D;&#x0A;   ip route-static 0.0.0.0  0.0.0.0  200.1.1.2&#x0D;&#x0A;&#x0D;&#x0A;   在SW1&#x0D;&#x0A;   ip route-static 0.0.0.0 0.0.0.0 192.168.30.253" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="789" top="369" right="1367" bottom="526" content="2、在R1 配置 acl , nat &#x0D;&#x0A;&#x0D;&#x0A;   acl  2000&#x0D;&#x0A;      rule  permit source  192.168.10.0 0.0.0.255&#x0D;&#x0A;&#x0D;&#x0A;   nat address-group 1 200.1.1.3 200.1.1.9   //创建地址池&#x0D;&#x0A;   interface  g0/0/1&#x0D;&#x0A;      nat outbound 2000 address-group 1      //通过地址池方式实现nat&#x0D;&#x0A;      nat server protocol tcp global 200.1.1.6 www inside 192.168.30.250 www&#x0D;&#x0A; " fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="787" top="516" right="965" bottom="564" content="3、在R1 查看 nat 配置 &#x0D;&#x0A; &#x0D;&#x0A;display  nat  outbound" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="793" top="609" right="1235" bottom="626" content="4、在pc1 、pc2 测试 到达 外网200.1.1.2 ,202.1.1.2 的连通性" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="794" top="676" right="1009" bottom="724" content="5、在R1 查看 nat 转换 的会话&#x0D;&#x0A;&#x0D;&#x0A;display  nat  session all" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="207" top="60" right="611" bottom="92" content="动态地址转换NAT  （地址池方式）&#x0D;&#x0A;将内网服务器通过地址映射（NAT Server 方式）发布到外网" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="421" top="390" right="553" bottom="407" content="192.168.30.250/28" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
    </txttips>
</topo>
