<?xml version="1.0" encoding="UNICODE" ?>
<topo version="1.2.00.510">
    <devices>
        <dev id="F0B57B87-500E-46d6-B5D2-59EE2B7A246A" name="PC3" poe="0" model="PC" settings=" -simpc_ip 172.16.1.2  -simpc_mask 255.255.255.0  -simpc_gateway 172.16.1.1  -simpc_mac 54-89-98-19-0A-C9  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-19-0A-C9" com_port="0" bootmode="0" cx="482.000000" cy="107.000000" edit_left="509" edit_top="161">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="D7B495CC-FF9D-4f45-9F76-55DFD5CB55C1" name="LSW2" poe="0" model="S5700" settings="" system_mac="4C-1F-CC-44-7C-44" com_port="2001" bootmode="0" cx="316.000000" cy="234.000000" edit_left="343" edit_top="288">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="24" />
            </slot>
        </dev>
        <dev id="0182D7D6-46D1-42b0-B72A-379DA6C6F6BF" name="PC1" poe="0" model="PC" settings=" -simpc_ip 192.168.10.2  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.10.1  -simpc_mac 54-89-98-F5-21-A1  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-F5-21-A1" com_port="0" bootmode="0" cx="269.000000" cy="367.000000" edit_left="296" edit_top="421">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="D4984B76-3AE3-49bd-B3FF-C58C38CCF29C" name="PC2" poe="0" model="PC" settings=" -simpc_ip 192.168.20.2  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.20.1  -simpc_mac 54-89-98-14-03-50  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-14-03-50" com_port="0" bootmode="0" cx="383.000000" cy="365.000000" edit_left="410" edit_top="419">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="FD10B352-762C-44c7-AD22-C0632FDEDB8E" name="FW1" poe="0" model="USG5500" settings="" system_mac="" com_port="2000" bootmode="0" cx="320.000000" cy="109.000000" edit_left="347" edit_top="163">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="9" />
            </slot>
        </dev>
    </devices>
    <lines>
        <line srcDeviceID="D7B495CC-FF9D-4f45-9F76-55DFD5CB55C1" destDeviceID="FD10B352-762C-44c7-AD22-C0632FDEDB8E">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="1" srcBoundRect_X="344.381165" srcBoundRect_Y="217.838333" srcOffset_X="13.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="1" tarBoundRect_X="345.618835" tarBoundRect_Y="179.161667" tarOffset_X="10.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="D7B495CC-FF9D-4f45-9F76-55DFD5CB55C1" destDeviceID="0182D7D6-46D1-42b0-B72A-379DA6C6F6BF">
            <interfacePair lineName="Copper" srcIndex="1" srcBoundRectIsMoved="1" srcBoundRect_X="328.611572" srcBoundRect_Y="301.716217" srcOffset_X="-65.000000" srcOffset_Y="-6.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="310.388428" tarBoundRect_Y="353.283783" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="D7B495CC-FF9D-4f45-9F76-55DFD5CB55C1" destDeviceID="D4984B76-3AE3-49bd-B3FF-C58C38CCF29C">
            <interfacePair lineName="Copper" srcIndex="2" srcBoundRectIsMoved="1" srcBoundRect_X="362.663757" srcBoundRect_Y="299.447021" srcOffset_X="15.000000" srcOffset_Y="-3.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="390.336243" tarBoundRect_Y="353.552979" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="FD10B352-762C-44c7-AD22-C0632FDEDB8E" destDeviceID="F0B57B87-500E-46d6-B5D2-59EE2B7A246A">
            <interfacePair lineName="Copper" srcIndex="1" srcBoundRectIsMoved="0" srcBoundRect_X="390.180481" srcBoundRect_Y="135.466904" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="465.819519" tarBoundRect_Y="134.533096" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
    </lines>
    <shapes />
    <txttips>
        <txttip left="493" top="73" right="572" bottom="90" content="172.16.1.2" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="257" top="445" right="352" bottom="462" content="192.168.10.2" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="415" top="449" right="510" bottom="466" content="192.168.20.2" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="648" top="115" right="946" bottom="366" content="将接口加入到安全区域&#x0D;&#x0A;firewall zone trust&#x0D;&#x0A; set priority 85&#x0D;&#x0A; add interface GigabitEthernet0/0/0&#x0D;&#x0A;#&#x0D;&#x0A;firewall zone untrust&#x0D;&#x0A; set priority 5&#x0D;&#x0A; add interface GigabitEthernet0/0/1&#x0D;&#x0A;&#x0D;&#x0A;通过域间策略实现数据包的过滤&#x0D;&#x0A;&#x0D;&#x0A;policy interzone trust untrust outbound&#x0D;&#x0A; policy 1&#x0D;&#x0A;  action permit&#x0D;&#x0A;  policy source 192.168.10.0 mask 24&#x0D;&#x0A;" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
    </txttips>
</topo>
