<?xml version="1.0" encoding="UNICODE" ?>
<topo version="1.2.00.510">
    <devices>
        <dev id="9964882A-F5AE-4d0b-B752-06CB976DB78B" name="PC1" poe="0" model="PC" settings=" -simpc_ip 0.0.0.0  -simpc_mask 0.0.0.0  -simpc_gateway 0.0.0.0  -simpc_mac 54-89-98-20-4B-52  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-20-4B-52" com_port="0" bootmode="0" cx="204.000000" cy="370.000000" edit_left="231" edit_top="424">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="E0FEF6A4-1CDC-4bca-BB7B-43256135E00E" name="PC4" poe="0" model="PC" settings=" -simpc_ip 192.168.20.2  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.20.254  -simpc_mac 54-89-98-AB-29-C1  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-AB-29-C1" com_port="0" bootmode="0" cx="490.000000" cy="368.000000" edit_left="517" edit_top="422">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="AFC6DFBE-25FE-49f9-8A23-BBFDA867FB2F" name="PC2" poe="0" model="PC" settings=" -simpc_ip 192.168.10.2  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.10.254  -simpc_mac 54-89-98-DB-18-C4  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-DB-18-C4" com_port="0" bootmode="0" cx="341.000000" cy="370.000000" edit_left="368" edit_top="424">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="AF8261BF-D04F-4713-8A3E-005FE4460D74" name="PC3" poe="0" model="PC" settings=" -simpc_ip 192.168.20.1  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.20.254  -simpc_mac 54-89-98-B6-0D-55  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-B6-0D-55" com_port="0" bootmode="0" cx="530.000000" cy="95.000000" edit_left="557" edit_top="149">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="42A447F7-A097-49fe-BB9C-305F78E6765E" name="LSW2" poe="0" model="S3700" settings="" system_mac="4C-1F-CC-37-7F-F9" com_port="2001" bootmode="0" cx="310.000000" cy="243.000000" edit_left="337" edit_top="297">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="22" />
                <interface sztype="Ethernet" interfacename="GE" count="2" />
            </slot>
        </dev>
        <dev id="B4284414-7CC4-46c5-B379-73C3C67135AC" name="LSW1" poe="0" model="S5700" settings="" system_mac="4C-1F-CC-99-43-C1" com_port="2000" bootmode="0" cx="309.000000" cy="93.000000" edit_left="336" edit_top="147">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="24" />
            </slot>
        </dev>
    </devices>
    <lines>
        <line srcDeviceID="9964882A-F5AE-4d0b-B752-06CB976DB78B" destDeviceID="42A447F7-A097-49fe-BB9C-305F78E6765E">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="258.671234" srcBoundRect_Y="363.846710" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="309.328766" tarBoundRect_Y="303.153290" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="AFC6DFBE-25FE-49f9-8A23-BBFDA867FB2F" destDeviceID="42A447F7-A097-49fe-BB9C-305F78E6765E">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="357.759735" srcBoundRect_Y="355.047943" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="1" tarBoundRectIsMoved="0" tarBoundRect_X="347.240265" tarBoundRect_Y="311.952057" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="42A447F7-A097-49fe-BB9C-305F78E6765E" destDeviceID="B4284414-7CC4-46c5-B379-73C3C67135AC">
            <interfacePair lineName="Copper" srcIndex="22" srcBoundRectIsMoved="0" srcBoundRect_X="336.712128" srcBoundRect_Y="226.817200" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="22" tarBoundRectIsMoved="0" tarBoundRect_X="336.287872" tarBoundRect_Y="163.182800" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
            <interfacePair lineName="Copper" srcIndex="23" srcBoundRectIsMoved="0" srcBoundRect_X="348.712128" srcBoundRect_Y="214.817200" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="23" tarBoundRectIsMoved="0" tarBoundRect_X="348.287872" tarBoundRect_Y="151.182800" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="B4284414-7CC4-46c5-B379-73C3C67135AC" destDeviceID="AF8261BF-D04F-4713-8A3E-005FE4460D74">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="379.182007" srcBoundRect_Y="120.390785" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="513.817993" tarBoundRect_Y="121.609215" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="42A447F7-A097-49fe-BB9C-305F78E6765E" destDeviceID="E0FEF6A4-1CDC-4bca-BB7B-43256135E00E">
            <interfacePair lineName="Copper" srcIndex="9" srcBoundRectIsMoved="0" srcBoundRect_X="372.469849" srcBoundRect_Y="294.631836" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="481.530151" tarBoundRect_Y="370.368164" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
    </lines>
    <shapes />
    <txttips>
        <txttip left="303" top="36" right="745" bottom="53" content="3虚拟局域网vlan-链路聚合 配置,增加链路带宽，提高链路可靠性" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="367" top="134" right="401" bottom="151" content="5700" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="366" top="260" right="400" bottom="277" content="3700" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="153" top="90" right="285" bottom="169" content="vlan10 ：&#x0D;&#x0A;192.168.10.254/24&#x0D;&#x0A;vlan20:&#x0D;&#x0A;192.168.20.254/24&#x0D;&#x0A;" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="180" top="449" right="297" bottom="466" content="192.168.10.1/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="339" top="453" right="456" bottom="470" content="192.168.10.2/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="601" top="117" right="718" bottom="134" content="192.168.20.1/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="491" top="453" right="608" bottom="470" content="192.168.20.2/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="370" top="204" right="434" bottom="221" content="链路聚合" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="249" top="287" right="298" bottom="304" content="e0/0/1" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="394" top="289" right="451" bottom="306" content="e0/0/10" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="273" top="227" right="322" bottom="244" content="g0/0/1" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="357" top="234" right="406" bottom="251" content="g0/0/2" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
    </txttips>
</topo>
