<?xml version="1.0" encoding="UNICODE" ?>
<topo version="1.2.00.510">
    <devices>
        <dev id="E5353DEC-2CE6-4fc0-A1DE-44FC2646D165" name="PC1" poe="0" model="PC" settings=" -simpc_ip 0.0.0.0  -simpc_mask 0.0.0.0  -simpc_gateway 0.0.0.0  -simpc_mac 54-89-98-B0-3E-33  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-B0-3E-33" com_port="0" bootmode="0" cx="103.000000" cy="350.000000" edit_left="130" edit_top="404">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="8C930BE2-6DB5-40a2-AE29-F74EFABB201B" name="PC2" poe="0" model="PC" settings=" -simpc_ip 0.0.0.0  -simpc_mask 0.0.0.0  -simpc_gateway 0.0.0.0  -simpc_mac 54-89-98-64-02-98  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-64-02-98" com_port="0" bootmode="0" cx="315.000000" cy="347.000000" edit_left="342" edit_top="401">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="C4312C3E-7992-4b45-A20A-76A3A12F71BC" name="LSW2" poe="0" model="S3700" settings="" system_mac="4C-1F-CC-F7-2D-E6" com_port="2001" bootmode="0" cx="102.000000" cy="215.000000" edit_left="129" edit_top="269">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="22" />
                <interface sztype="Ethernet" interfacename="GE" count="2" />
            </slot>
        </dev>
        <dev id="A0DAEDC7-070B-4623-BB15-A7E913287317" name="LSW3" poe="0" model="S3700" settings="" system_mac="4C-1F-CC-43-71-08" com_port="2002" bootmode="0" cx="302.000000" cy="216.000000" edit_left="329" edit_top="270">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="22" />
                <interface sztype="Ethernet" interfacename="GE" count="2" />
            </slot>
        </dev>
        <dev id="092B566C-58AE-4afd-A003-28C65E854381" name="LSW1" poe="0" model="S5700" settings="" system_mac="4C-1F-CC-DB-6A-3E" com_port="2000" bootmode="0" cx="215.000000" cy="83.000000" edit_left="242" edit_top="137">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="24" />
            </slot>
        </dev>
    </devices>
    <lines>
        <line srcDeviceID="092B566C-58AE-4afd-A003-28C65E854381" destDeviceID="C4312C3E-7992-4b45-A20A-76A3A12F71BC">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="213.916855" srcBoundRect_Y="142.805099" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="157.083145" tarBoundRect_Y="209.194901" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="092B566C-58AE-4afd-A003-28C65E854381" destDeviceID="A0DAEDC7-070B-4623-BB15-A7E913287317">
            <interfacePair lineName="Copper" srcIndex="1" srcBoundRectIsMoved="0" srcBoundRect_X="265.639618" srcBoundRect_Y="146.138718" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="305.360382" tarBoundRect_Y="206.861282" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="C4312C3E-7992-4b45-A20A-76A3A12F71BC" destDeviceID="A0DAEDC7-070B-4623-BB15-A7E913287317">
            <interfacePair lineName="Copper" srcIndex="1" srcBoundRectIsMoved="0" srcBoundRect_X="172.183228" srcBoundRect_Y="242.215912" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="1" tarBoundRectIsMoved="0" tarBoundRect_X="285.816772" tarBoundRect_Y="242.784088" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="C4312C3E-7992-4b45-A20A-76A3A12F71BC" destDeviceID="E5353DEC-2CE6-4fc0-A1DE-44FC2646D165">
            <interfacePair lineName="Copper" srcIndex="2" srcBoundRectIsMoved="0" srcBoundRect_X="129.319870" srcBoundRect_Y="285.182587" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="129.680130" tarBoundRect_Y="333.817413" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="A0DAEDC7-070B-4623-BB15-A7E913287317" destDeviceID="8C930BE2-6DB5-40a2-AE29-F74EFABB201B">
            <interfacePair lineName="Copper" srcIndex="2" srcBoundRectIsMoved="0" srcBoundRect_X="333.264465" srcBoundRect_Y="285.972687" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="337.735535" tarBoundRect_Y="331.027313" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
    </lines>
    <shapes />
    <txttips>
        <txttip left="188" top="27" right="298" bottom="44" content="生成树协议配置" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="583" top="66" right="632" bottom="83" content="步骤：" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="586" top="103" right="1013" bottom="135" content="1、查看生成树信息，判断哪台交换机是根桥，哪个接口被阻塞&#x0D;&#x0A;   display stp" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="155" top="117" right="204" bottom="134" content="G0/0/1" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="274" top="122" right="323" bottom="139" content="G0/0/2" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="129" top="194" right="178" bottom="211" content="E0/0/1" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="168" top="259" right="217" bottom="276" content="E0/0/2" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="313" top="196" right="362" bottom="213" content="E0/0/1" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="0" top="233" right="110" bottom="265" content="4c1f-ccf7-2de6&#x0D;&#x0A;" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="205" top="72" right="315" bottom="89" content="4c1f-ccdb-6a3e" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="372" top="238" right="482" bottom="255" content="4c1f-cc43-7108" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="61" top="444" right="201" bottom="461" content="1最小的RID成为根桥" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="584" top="229" right="739" bottom="261" content="3、配置LSW1作为根桥&#x0D;&#x0A;   stp root primay " fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="584" top="290" right="792" bottom="307" content="4、再次判读哪个端口被阻塞？" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="579" top="343" right="870" bottom="391" content="5、设置连接电脑的交换机接口为边缘端口&#x0D;&#x0A;   int e0/0/3&#x0D;&#x0A;   stp edged-port enable" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="588" top="175" right="788" bottom="207" content="2、配置stp 的模式&#x0D;&#x0A;  stp mode stp |rstp |mstp" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
    </txttips>
</topo>
