<?xml version="1.0" encoding="UNICODE" ?>
<topo version="1.2.00.510">
    <devices>
        <dev id="CF1DF27F-8BB0-471e-91F7-F2717BA0553F" name="PC1" poe="0" model="PC" settings=" -simpc_ip 0.0.0.0  -simpc_mask 0.0.0.0  -simpc_gateway 0.0.0.0  -simpc_mac 54-89-98-FF-33-65  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-FF-33-65" com_port="0" bootmode="0" cx="131.000000" cy="372.000000" edit_left="158" edit_top="426">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="96FCFC60-5AB8-407e-8C34-7B203C8EDC35" name="PC3" poe="0" model="PC" settings=" -simpc_ip 0.0.0.0  -simpc_mask 0.0.0.0  -simpc_gateway 0.0.0.0  -simpc_mac 54-89-98-80-3F-B8  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-80-3F-B8" com_port="0" bootmode="0" cx="519.000000" cy="376.000000" edit_left="546" edit_top="430">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="1A718709-0A22-4b29-8455-D67B278085A3" name="PC2" poe="0" model="PC" settings=" -simpc_ip 0.0.0.0  -simpc_mask 0.0.0.0  -simpc_gateway 0.0.0.0  -simpc_mac 54-89-98-34-7B-96  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-34-7B-96" com_port="0" bootmode="0" cx="325.000000" cy="369.000000" edit_left="352" edit_top="423">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="7B2C4762-2E2B-4f86-A821-B67A8EF1D3E9" name="AR1" poe="0" model="AR1220" settings="" system_mac="00-E0-FC-04-1B-97" com_port="2000" bootmode="0" cx="128.000000" cy="208.000000" edit_left="155" edit_top="262">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="2" />
                <interface sztype="Ethernet" interfacename="Ethernet" count="8" />
                <interface sztype="Serial" interfacename="Serial" count="2" />
            </slot>
            <slot isMainBoard="0" id="0" type="521" />
        </dev>
        <dev id="26C1E963-C69C-4e5d-9426-A3A37E9545CC" name="AR3" poe="0" model="AR1220" settings="" system_mac="00-E0-FC-67-1F-DB" com_port="2002" bootmode="0" cx="516.000000" cy="203.000000" edit_left="543" edit_top="257">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="2" />
                <interface sztype="Ethernet" interfacename="Ethernet" count="8" />
                <interface sztype="Serial" interfacename="Serial" count="2" />
            </slot>
            <slot isMainBoard="0" id="0" type="521" />
        </dev>
        <dev id="CAA11BAC-1A3B-4dda-AFE4-79FE1761A59D" name="AR2" poe="0" model="AR1220" settings="" system_mac="00-E0-FC-D6-2A-C0" com_port="2001" bootmode="0" cx="317.000000" cy="77.000000" edit_left="344" edit_top="131">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="2" />
                <interface sztype="Ethernet" interfacename="Ethernet" count="8" />
                <interface sztype="Serial" interfacename="Serial" count="2" />
            </slot>
            <slot isMainBoard="0" id="0" type="521" />
        </dev>
    </devices>
    <lines>
        <line srcDeviceID="CF1DF27F-8BB0-471e-91F7-F2717BA0553F" destDeviceID="7B2C4762-2E2B-4f86-A821-B67A8EF1D3E9">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="157.210190" srcBoundRect_Y="355.823456" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="155.789810" tarBoundRect_Y="278.176544" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="7B2C4762-2E2B-4f86-A821-B67A8EF1D3E9" destDeviceID="CAA11BAC-1A3B-4dda-AFE4-79FE1761A59D">
            <interfacePair lineName="Serial" srcIndex="10" srcBoundRectIsMoved="0" srcBoundRect_X="190.491837" srcBoundRect_Y="210.399841" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="10" tarBoundRectIsMoved="0" tarBoundRect_X="308.508179" tarBoundRect_Y="128.600159" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="1A718709-0A22-4b29-8455-D67B278085A3" destDeviceID="CAA11BAC-1A3B-4dda-AFE4-79FE1761A59D">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="350.817322" srcBoundRect_Y="352.832428" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="345.182678" tarBoundRect_Y="147.167572" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="96FCFC60-5AB8-407e-8C34-7B203C8EDC35" destDeviceID="26C1E963-C69C-4e5d-9426-A3A37E9545CC">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="545.251282" srcBoundRect_Y="359.822723" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="543.748718" tarBoundRect_Y="273.177277" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="CAA11BAC-1A3B-4dda-AFE4-79FE1761A59D" destDeviceID="26C1E963-C69C-4e5d-9426-A3A37E9545CC">
            <interfacePair lineName="Serial" srcIndex="11" srcBoundRectIsMoved="0" srcBoundRect_X="380.485229" srcBoundRect_Y="127.101204" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="11" tarBoundRectIsMoved="0" tarBoundRect_X="506.514771" tarBoundRect_Y="206.898804" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
    </lines>
    <shapes />
    <txttips>
        <txttip left="110" top="158" right="197" bottom="190" content="S1/0/0&#x0D;&#x0A;10.1.2.1/30" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="223" top="83" right="310" bottom="115" content="s1/0/0&#x0D;&#x0A;10.1.2.2/30" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="385" top="88" right="472" bottom="120" content="s1/0/1&#x0D;&#x0A;10.1.2.5/30" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="496" top="141" right="583" bottom="173" content="s1/0/1&#x0D;&#x0A;10.1.2.6/30" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="171" top="276" right="303" bottom="308" content="g0/0/0/&#x0D;&#x0A;192.168.10.254/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="354" top="176" right="486" bottom="208" content="g0/0/0&#x0D;&#x0A;192.168.20.254/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="562" top="271" right="694" bottom="303" content="g0/0/0&#x0D;&#x0A;192.168.30.254/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="291" top="25" right="408" bottom="42" content="10 ospf路由配置" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="114" top="457" right="231" bottom="474" content="192.168.10.1/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="328" top="460" right="445" bottom="477" content="192.168.20.1/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="531" top="457" right="648" bottom="474" content="192.168.30.1/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="750" top="90" right="1011" bottom="169" content="R1:&#x0D;&#x0A;ospf 1&#x0D;&#x0A;   area 0&#x0D;&#x0A;   network 192.168.10.0 0.0.0.255&#x0D;&#x0A;   network 10.1.2.0 0.0.0.3" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="752" top="205" right="1005" bottom="300" content="R2:&#x0D;&#x0A;ospf 1&#x0D;&#x0A;   area 0&#x0D;&#x0A;   network 192.168.20.0 0.0.0.255&#x0D;&#x0A;   network 10.1.2.0 0.0.0.3&#x0D;&#x0A;   network 10.1.2.4 0.0.0.3" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="755" top="325" right="1008" bottom="404" content="R3:&#x0D;&#x0A;ospf 1&#x0D;&#x0A;   area 0&#x0D;&#x0A;   network 192.168.30.0 0.0.0.255&#x0D;&#x0A;   network 10.1.2.4 0.0.0.3" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="760" top="28" right="839" bottom="45" content="配置步骤：" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="752" top="429" right="945" bottom="477" content="查看IP 路由表&#x0D;&#x0A;&#x0D;&#x0A; display ip routing-table" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
    </txttips>
</topo>
