<?xml version="1.0" encoding="UNICODE" ?>
<topo version="1.2.00.510">
    <devices>
        <dev id="96FCFC60-5AB8-407e-8C34-7B203C8EDC35" name="PC3" poe="0" model="PC" settings=" -simpc_ip 0.0.0.0  -simpc_mask 0.0.0.0  -simpc_gateway 0.0.0.0  -simpc_mac 54-89-98-80-3F-B8  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-80-3F-B8" com_port="0" bootmode="1" cx="664.000000" cy="369.000000" edit_left="691" edit_top="423">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="CAA11BAC-1A3B-4dda-AFE4-79FE1761A59D" name="AR2" poe="0" model="AR1220" settings="" system_mac="00-E0-FC-D6-2A-C0" com_port="2001" bootmode="0" cx="374.000000" cy="196.000000" edit_left="401" edit_top="250">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="2" />
                <interface sztype="Ethernet" interfacename="Ethernet" count="8" />
                <interface sztype="Serial" interfacename="Serial" count="2" />
            </slot>
            <slot isMainBoard="0" id="0" type="521" />
        </dev>
        <dev id="CF1DF27F-8BB0-471e-91F7-F2717BA0553F" name="PC1" poe="0" model="PC" settings=" -simpc_ip 0.0.0.0  -simpc_mask 0.0.0.0  -simpc_gateway 0.0.0.0  -simpc_mac 54-89-98-FF-33-65  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-FF-33-65" com_port="0" bootmode="1" cx="80.000000" cy="382.000000" edit_left="107" edit_top="436">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="7B2C4762-2E2B-4f86-A821-B67A8EF1D3E9" name="AR1" poe="0" model="AR1220" settings="" system_mac="00-E0-FC-04-1B-97" com_port="2000" bootmode="1" cx="78.000000" cy="195.000000" edit_left="105" edit_top="249">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="2" />
                <interface sztype="Ethernet" interfacename="Ethernet" count="8" />
                <interface sztype="Serial" interfacename="Serial" count="2" />
            </slot>
            <slot isMainBoard="0" id="0" type="521" />
        </dev>
        <dev id="1A718709-0A22-4b29-8455-D67B278085A3" name="PC2" poe="0" model="PC" settings=" -simpc_ip 0.0.0.0  -simpc_mask 0.0.0.0  -simpc_gateway 0.0.0.0  -simpc_mac 54-89-98-34-7B-96  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-34-7B-96" com_port="0" bootmode="1" cx="374.000000" cy="371.000000" edit_left="401" edit_top="425">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="26C1E963-C69C-4e5d-9426-A3A37E9545CC" name="AR3" poe="0" model="AR1220" settings="" system_mac="00-E0-FC-67-1F-DB" com_port="2002" bootmode="1" cx="661.000000" cy="196.000000" edit_left="688" edit_top="250">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="2" />
                <interface sztype="Ethernet" interfacename="Ethernet" count="8" />
                <interface sztype="Serial" interfacename="Serial" count="2" />
            </slot>
            <slot isMainBoard="0" id="0" type="521" />
        </dev>
    </devices>
    <lines>
        <line srcDeviceID="CF1DF27F-8BB0-471e-91F7-F2717BA0553F" destDeviceID="7B2C4762-2E2B-4f86-A821-B67A8EF1D3E9">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="106.538170" srcBoundRect_Y="365.818695" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="105.461830" tarBoundRect_Y="265.181305" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="7B2C4762-2E2B-4f86-A821-B67A8EF1D3E9" destDeviceID="CAA11BAC-1A3B-4dda-AFE4-79FE1761A59D">
            <interfacePair lineName="Serial" srcIndex="10" srcBoundRectIsMoved="0" srcBoundRect_X="148.183517" srcBoundRect_Y="222.145889" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="10" tarBoundRectIsMoved="0" tarBoundRect_X="357.816467" tarBoundRect_Y="222.854111" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="CAA11BAC-1A3B-4dda-AFE4-79FE1761A59D" destDeviceID="26C1E963-C69C-4e5d-9426-A3A37E9545CC">
            <interfacePair lineName="Serial" srcIndex="11" srcBoundRectIsMoved="0" srcBoundRect_X="444.183777" srcBoundRect_Y="223.000000" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="10" tarBoundRectIsMoved="0" tarBoundRect_X="644.816223" tarBoundRect_Y="223.000000" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="1A718709-0A22-4b29-8455-D67B278085A3" destDeviceID="CAA11BAC-1A3B-4dda-AFE4-79FE1761A59D">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="401.000000" srcBoundRect_Y="354.816223" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="401.000000" tarBoundRect_Y="266.183777" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="96FCFC60-5AB8-407e-8C34-7B203C8EDC35" destDeviceID="26C1E963-C69C-4e5d-9426-A3A37E9545CC">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="690.251282" srcBoundRect_Y="352.822723" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="688.748718" tarBoundRect_Y="266.177277" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
    </lines>
    <shapes />
    <txttips>
        <txttip left="59" top="155" right="146" bottom="187" content="S1/0/0&#x0D;&#x0A;10.1.2.1/30" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="279" top="181" right="366" bottom="213" content="s1/0/0&#x0D;&#x0A;10.1.2.2/30" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="443" top="180" right="530" bottom="212" content="s1/0/1&#x0D;&#x0A;10.1.2.5/30" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="641" top="134" right="728" bottom="166" content="s1/0/1&#x0D;&#x0A;10.1.2.6/30" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="120" top="255" right="252" bottom="287" content="g0/0/0/&#x0D;&#x0A;192.168.10.254/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="411" top="295" right="543" bottom="327" content="g0/0/0&#x0D;&#x0A;192.168.20.254/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="707" top="264" right="839" bottom="296" content="g0/0/0&#x0D;&#x0A;192.168.30.254/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="291" top="25" right="386" bottom="42" content="静态路由配置" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="63" top="454" right="180" bottom="471" content="192.168.10.1/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="352" top="453" right="469" bottom="470" content="192.168.20.1/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="640" top="452" right="757" bottom="469" content="192.168.30.1/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="986" top="102" right="1322" bottom="134" content="R1:&#x0D;&#x0A;ip route-static 0.0.0.0   0.0.0.0   10.1.2.2" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="988" top="172" right="1377" bottom="220" content="R2:&#x0D;&#x0A;ip route-static 192.168.10.0 255.255.255   10.1.2.1&#x0D;&#x0A;ip route-static 192.168.30.0 255.255.255   10.1.2.6" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="992" top="262" right="1328" bottom="294" content="R3:&#x0D;&#x0A;ip route-static 0.0.0.0   0.0.0.0   10.1.2.5" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="996" top="40" right="1075" bottom="57" content="配置步骤：" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="991" top="343" right="1184" bottom="391" content="查看IP 路由表&#x0D;&#x0A;&#x0D;&#x0A; display ip routing-table" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
    </txttips>
</topo>
