<?xml version="1.0" encoding="UNICODE" ?>
<topo version="1.2.00.510">
    <devices>
        <dev id="E8275AE8-A4C6-465e-B4F6-B793884D51EC" name="PC4" poe="0" model="PC" settings=" -simpc_ip 192.168.30.2  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.30.254  -simpc_mac 54-89-98-90-79-2E  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-90-79-2E" com_port="0" bootmode="0" cx="512.000000" cy="271.000000" edit_left="539" edit_top="325">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="8CD26B30-8001-4bbe-B24B-50EDE5307646" name="PC1" poe="0" model="PC" settings=" -simpc_ip 192.168.10.1  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.10.254  -simpc_mac 54-89-98-F7-3F-7B  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-F7-3F-7B" com_port="0" bootmode="0" cx="91.000000" cy="257.000000" edit_left="118" edit_top="311">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="894D940E-C695-4113-92D8-951D8B9ED22F" name="PC3" poe="0" model="PC" settings=" -simpc_ip 192.168.20.2  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.20.254  -simpc_mac 54-89-98-69-39-58  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-69-39-58" com_port="0" bootmode="0" cx="393.000000" cy="385.000000" edit_left="420" edit_top="439">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="A791B153-A5BC-4406-9077-51FD9F233BD9" name="LSW1" poe="0" model="S5700" settings="" system_mac="4C-1F-CC-6D-74-D9" com_port="2000" bootmode="0" cx="319.000000" cy="168.000000" edit_left="346" edit_top="222">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="24" />
            </slot>
        </dev>
        <dev id="4C9D192C-6E7A-49fe-9EA8-10F6A2DBC8A5" name="PC2" poe="0" model="PC" settings=" -simpc_ip 192.168.10.2  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.10.254  -simpc_mac 54-89-98-BC-35-02  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-BC-35-02" com_port="0" bootmode="0" cx="218.000000" cy="373.000000" edit_left="245" edit_top="427">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
    </devices>
    <lines>
        <line srcDeviceID="8CD26B30-8001-4bbe-B24B-50EDE5307646" destDeviceID="A791B153-A5BC-4406-9077-51FD9F233BD9">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="158.227570" srcBoundRect_Y="268.297119" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="305.772430" tarBoundRect_Y="210.702866" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="4C9D192C-6E7A-49fe-9EA8-10F6A2DBC8A5" destDeviceID="A791B153-A5BC-4406-9077-51FD9F233BD9">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="264.085266" srcBoundRect_Y="361.262543" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="1" tarBoundRectIsMoved="0" tarBoundRect_X="326.914734" tarBoundRect_Y="233.737442" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="894D940E-C695-4113-92D8-951D8B9ED22F" destDeviceID="A791B153-A5BC-4406-9077-51FD9F233BD9">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="406.061890" srcBoundRect_Y="371.127441" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="9" tarBoundRectIsMoved="0" tarBoundRect_X="359.938110" tarBoundRect_Y="235.872574" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="E8275AE8-A4C6-465e-B4F6-B793884D51EC" destDeviceID="A791B153-A5BC-4406-9077-51FD9F233BD9">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="1" srcBoundRect_X="500.902130" srcBoundRect_Y="277.667969" srcOffset_X="18.000000" srcOffset_Y="53.000000" tarIndex="19" tarBoundRectIsMoved="0" tarBoundRect_X="384.097870" tarBoundRect_Y="215.332016" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
    </lines>
    <shapes />
    <txttips>
        <txttip left="63" top="218" right="180" bottom="250" content="vlan 10&#x0D;&#x0A;192.168.10.1/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="203" top="461" right="320" bottom="493" content="vlan10&#x0D;&#x0A;192.168.10.2/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="400" top="478" right="517" bottom="510" content="vlan 20&#x0D;&#x0A;192.168.20.2/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="522" top="232" right="639" bottom="264" content="vlan 30&#x0D;&#x0A;192.168.30.2/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="297" top="24" right="512" bottom="41" content="13流策略traffic-policy的配置" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="112" top="82" right="403" bottom="130" content="实现的目标：&#x0D;&#x0A;1、禁止vlan 10 与vlan 20 相互通信&#x0D;&#x0A;2、允许vlan 10 、vlan20 与 vlan30 通讯" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="166" top="547" right="774" bottom="814" content="配置过程：&#x0D;&#x0A;&#x0D;&#x0A;acl number 3001&#x0D;&#x0A; rule 5 deny ip source 192.168.10.0 0.0.0.255 destination 192.168.20.0 0.0.0.255&#x0D;&#x0A;#&#x0D;&#x0A;traffic classifier tc1 &#x0D;&#x0A; if-match acl 3001&#x0D;&#x0A;#&#x0D;&#x0A;traffic behavior tb1&#x0D;&#x0A; deny&#x0D;&#x0A;#&#x0D;&#x0A;traffic policy tp1&#x0D;&#x0A; classifier tc1 behavior tb1&#x0D;&#x0A;#&#x0D;&#x0A;vlan 10&#x0D;&#x0A; traffic-policy tp1 inbound  //流策略可以应用到 vlan 中，但acl只能应用到物理接口&#x0D;&#x0A;" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
    </txttips>
</topo>
