<?xml version="1.0" encoding="UNICODE" ?>
<topo version="1.2.00.510">
    <devices>
        <dev id="F65F6CA7-8EB1-403b-919B-F11E0883C726" name="PC1" poe="0" model="PC" settings=" -simpc_ip 192.168.10.1  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.10.254  -simpc_mac 54-89-98-C3-35-17  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-C3-35-17" com_port="0" bootmode="0" cx="207.000000" cy="328.000000" edit_left="234" edit_top="382">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="CB6159A4-F9EB-40de-AAFA-837DBCED8B6E" name="PC4" poe="0" model="PC" settings=" -simpc_ip 192.168.1.3  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.1.254  -simpc_mac 54-89-98-7C-11-D8  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-7C-11-D8" com_port="0" bootmode="0" cx="622.000000" cy="328.000000" edit_left="649" edit_top="382">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="8386FD50-7D2F-43e6-9670-D0AB38C3EC68" name="PC3" poe="0" model="PC" settings=" -simpc_ip 192.168.10.2  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.10.254  -simpc_mac 54-89-98-A4-0C-5D  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-A4-0C-5D" com_port="0" bootmode="0" cx="496.000000" cy="327.000000" edit_left="523" edit_top="381">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="3B76129E-786E-450b-BEB6-6CF561EE190D" name="LSW2" poe="0" model="S3700" settings="" system_mac="4C-1F-CC-D3-5F-14" com_port="2001" bootmode="0" cx="205.000000" cy="179.000000" edit_left="232" edit_top="233">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="22" />
                <interface sztype="Ethernet" interfacename="GE" count="2" />
            </slot>
        </dev>
        <dev id="B18EE635-BAAA-4d38-9CBD-D17F402B8035" name="LSW1" poe="0" model="S5700" settings="" system_mac="4C-1F-CC-AA-49-8F" com_port="2000" bootmode="0" cx="378.000000" cy="48.000000" edit_left="405" edit_top="102">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="24" />
            </slot>
        </dev>
        <dev id="BC8989B3-011C-4f76-9079-EDA307ED1DA3" name="LSW4" poe="0" model="S3700" settings="" system_mac="4C-1F-CC-1A-03-90" com_port="2003" bootmode="0" cx="532.000000" cy="195.000000" edit_left="559" edit_top="249">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="22" />
                <interface sztype="Ethernet" interfacename="GE" count="2" />
            </slot>
        </dev>
    </devices>
    <lines>
        <line srcDeviceID="B18EE635-BAAA-4d38-9CBD-D17F402B8035" destDeviceID="3B76129E-786E-450b-BEB6-6CF561EE190D">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="370.572754" srcBoundRect_Y="101.069183" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="266.427246" tarBoundRect_Y="179.930817" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="F65F6CA7-8EB1-403b-919B-F11E0883C726" destDeviceID="3B76129E-786E-450b-BEB6-6CF561EE190D">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="233.420410" srcBoundRect_Y="311.820129" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="1" tarBoundRectIsMoved="0" tarBoundRect_X="232.579590" tarBoundRect_Y="249.179871" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="8386FD50-7D2F-43e6-9670-D0AB38C3EC68" destDeviceID="BC8989B3-011C-4f76-9079-EDA307ED1DA3">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="534.362427" srcBoundRect_Y="312.337860" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="1" tarBoundRectIsMoved="0" tarBoundRect_X="547.637573" tarBoundRect_Y="263.662140" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="CB6159A4-F9EB-40de-AAFA-837DBCED8B6E" destDeviceID="BC8989B3-011C-4f76-9079-EDA307ED1DA3">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="624.798279" srcBoundRect_Y="319.235260" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="2" tarBoundRectIsMoved="0" tarBoundRect_X="583.201721" tarBoundRect_Y="257.764740" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="B18EE635-BAAA-4d38-9CBD-D17F402B8035" destDeviceID="BC8989B3-011C-4f76-9079-EDA307ED1DA3">
            <interfacePair lineName="Copper" srcIndex="1" srcBoundRectIsMoved="0" srcBoundRect_X="436.237213" srcBoundRect_Y="104.817345" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="527.762756" tarBoundRect_Y="192.182663" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
    </lines>
    <shapes />
    <txttips>
        <txttip left="335" top="16" right="520" bottom="33" content="配置GVRP实现VLAN自动注册" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="495" top="64" right="703" bottom="81" content="在交换机LSW1建立vlan 10、12" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="338" top="87" right="387" bottom="104" content="g0/0/1" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="264" top="185" right="313" bottom="202" content="e0/0/1" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="415" top="191" right="464" bottom="208" content="e0/0/1" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="229" top="148" right="278" bottom="165" content="normal" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="305" top="61" right="347" bottom="78" content="fixed" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="529" top="165" right="601" bottom="182" content="forbidden" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="818" top="56" right="1351" bottom="245" content="GVRP 的端口注册模式有三种：Normal、Fixed 和Forbidden，各模式描述如下：&#x0D;&#x0A;&#x0D;&#x0A;?? Normal 模式：允许该端口动态注册、注销VLAN，传播动态VLAN 以及静态&#x0D;&#x0A;VLAN 信息。&#x0D;&#x0A;&#x0D;&#x0A;?? Fixed 模式：禁止该端口动态注册、注销VLAN，只传播静态VLAN 信息，不&#x0D;&#x0A;传播动态VLAN 信息。也就是说被设置为Fixed 模式的Trunk 口，即使允许所&#x0D;&#x0A;有VLAN 通过，实际通过的VLAN 也只能是手动配置的那部分。&#x0D;&#x0A;&#x0D;&#x0A;?? Forbidden 模式：禁止该端口动态注册、注销VLAN，不传播除VLAN 1 以外&#x0D;&#x0A;的任何的VLAN 信息。也就是说被配置为Forbidden 模式的Trunk 口，即使允&#x0D;&#x0A;许所有VLAN 通过，实际通过的VLAN 也只能是缺省VLAN，即VLAN 1" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="612" top="281" right="654" bottom="298" content="vlan1" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="242" top="286" right="291" bottom="318" content="vlan10&#x0D;&#x0A;" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="541" top="294" right="590" bottom="311" content="vlan10" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="444" top="88" right="493" bottom="105" content="normal" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="595" top="221" right="712" bottom="238" content=" 建立vlan10、13" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="88" top="200" right="167" bottom="217" content="建立vlan11" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="819" top="288" right="898" bottom="305" content="配置步骤：" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="822" top="331" right="1030" bottom="348" content="1、分别给三台交换机启用gvrp" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="825" top="378" right="1418" bottom="395" content="2、分别给连接交换机的端口设置trunk模式，并允许所有vlan通过，同时激活端口的gvrp" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="821" top="444" right="1089" bottom="461" content="3、按图中的要求给端口设置gvrp的模式" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="822" top="515" right="1120" bottom="532" content="4、分别在LSW1、LSW2、LSW3创建相应的vlan" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="821" top="578" right="1104" bottom="595" content="5、分别在LSW1、LSW2、LSW3观测vlan情况" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="189" top="413" right="306" bottom="430" content="192.168.10.1/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="456" top="406" right="573" bottom="423" content="192.168.10.2/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="634" top="407" right="744" bottom="424" content="192.168.1.3/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="423" top="45" right="593" bottom="62" content="vlan1:192.168.1.254/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="591" top="194" right="746" bottom="211" content="vlan1:192.168.1.2/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="824" top="635" right="1712" bottom="667" content="6、在LSW1配置vlan1接口IP地址为192。168.1.1/24，在LSW4配置vlan1 IP 地址为192.168.1.2/24，Pc4 IP地址为192.168.1.3/24 ，&#x0D;&#x0A;测试它们之间的连通性" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="825" top="713" right="1191" bottom="730" content="7、测试PC1 与 PC3 的连通性，解析为什么结果如此？" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
    </txttips>
</topo>
