<?xml version="1.0" encoding="UNICODE" ?>
<topo version="1.2.00.510">
    <devices>
        <dev id="1DEB3294-53F6-43cd-876B-2548A5870CD5" name="PC1" poe="0" model="PC" settings=" -simpc_ip 192.168.10.1  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.10.254  -simpc_mac 54-89-98-F6-07-2B  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-F6-07-2B" com_port="0" bootmode="0" cx="111.000000" cy="337.000000" edit_left="138" edit_top="391">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="9CEF4D0E-823A-41e4-9B16-D90B0AB511B7" name="PC2" poe="0" model="PC" settings=" -simpc_ip 192.168.20.1  -simpc_mask 255.255.255.0  -simpc_gateway 192.168.20.254  -simpc_mac 54-89-98-EF-1D-35  -simpc_mc_dstip 0.0.0.0  -simpc_mc_dstmac 00-00-00-00-00-00  -simpc_dns1 0.0.0.0  -simpc_dns2 0.0.0.0  -simpc_ipv6 ::  -simpc_prefix 128  -simpc_gatewayv6 ::  -simpc_dhcp_state 0  -simpc_dhcpv6_state 0  -simpc_dns_auto_state 0  -simpc_igmp_version 1  -simpc_group_ip_start 0.0.0.0  -simpc_src_ip_start 0.0.0.0  -simpc_group_num 0  -simpc_group_step 0  -simpc_src_num 0  -simpc_src_step 0  -simpc_type MODE_IS_INCLUDE " system_mac="54-89-98-EF-1D-35" com_port="0" bootmode="0" cx="260.000000" cy="342.000000" edit_left="287" edit_top="396">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="1" />
            </slot>
        </dev>
        <dev id="1360E073-0740-42af-85E1-E96381632BCE" name="LSW1" poe="0" model="S3700" settings="" system_mac="4C-1F-CC-5B-6A-FB" com_port="2001" bootmode="0" cx="181.000000" cy="216.000000" edit_left="208" edit_top="270">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="Ethernet" count="22" />
                <interface sztype="Ethernet" interfacename="GE" count="2" />
            </slot>
        </dev>
        <dev id="FD675CFE-E6E7-48b3-9727-A220936DA77D" name="AR1" poe="0" model="AR1220" settings="" system_mac="00-E0-FC-DD-5C-04" com_port="2000" bootmode="0" cx="184.000000" cy="93.000000" edit_left="211" edit_top="147">
            <slot number="slot17" isMainBoard="1">
                <interface sztype="Ethernet" interfacename="GE" count="2" />
                <interface sztype="Ethernet" interfacename="Ethernet" count="8" />
            </slot>
        </dev>
    </devices>
    <lines>
        <line srcDeviceID="1360E073-0740-42af-85E1-E96381632BCE" destDeviceID="1DEB3294-53F6-43cd-876B-2548A5870CD5">
            <interfacePair lineName="Copper" srcIndex="0" srcBoundRectIsMoved="0" srcBoundRect_X="186.375549" srcBoundRect_Y="280.379425" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="159.624451" tarBoundRect_Y="326.620575" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="1360E073-0740-42af-85E1-E96381632BCE" destDeviceID="9CEF4D0E-823A-41e4-9B16-D90B0AB511B7">
            <interfacePair lineName="Copper" srcIndex="9" srcBoundRectIsMoved="0" srcBoundRect_X="230.939529" srcBoundRect_Y="279.587097" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="264.060486" tarBoundRect_Y="332.412903" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
        <line srcDeviceID="1360E073-0740-42af-85E1-E96381632BCE" destDeviceID="FD675CFE-E6E7-48b3-9727-A220936DA77D">
            <interfacePair lineName="Copper" srcIndex="22" srcBoundRectIsMoved="0" srcBoundRect_X="209.052948" srcBoundRect_Y="199.829071" srcOffset_X="0.000000" srcOffset_Y="0.000000" tarIndex="0" tarBoundRectIsMoved="0" tarBoundRect_X="209.947052" tarBoundRect_Y="163.170929" tarOffset_X="0.000000" tarOffset_Y="0.000000" />
        </line>
    </lines>
    <shapes />
    <txttips>
        <txttip left="173" top="34" right="268" bottom="51" content="单臂路由配置" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="411" top="82" right="460" bottom="99" content="步骤：" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="415" top="118" right="615" bottom="150" content="1、在交换机创建vlan 10 20&#x0D;&#x0A;   vlan batch 10 20" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="417" top="173" right="731" bottom="283" content="2、在交换机配置trunk端口、access端口&#x0D;&#x0A;   interface g0/0/1&#x0D;&#x0A;      port  link-type  trunk&#x0D;&#x0A;      port  trunk  allow-pass  vlan  all&#x0D;&#x0A;   interface e0/0/1&#x0D;&#x0A;      port  link-type  access&#x0D;&#x0A;      port  default  vlan 10" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="413" top="291" right="893" bottom="433" content="3、在路由器AR1创建 子接口，封装dot1Q ，配置IP地址，启用ARP广播&#x0D;&#x0A;   interface g0/0/0.10&#x0D;&#x0A;      dot1Q  termination  vid 10&#x0D;&#x0A;      arp broadcast enable&#x0D;&#x0A;      ip  address 192.168.10.254 24&#x0D;&#x0A;   interface g0/0/0.20&#x0D;&#x0A;      dot1Q  termination  vid 20&#x0D;&#x0A;      arp broadcast enable&#x0D;&#x0A;      ip  address  192.168.20.254 24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="48" top="95" right="180" bottom="127" content="G0/0/0.10:&#x0D;&#x0A;192.168.10.254/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="74" top="412" right="191" bottom="444" content="vlan10&#x0D;&#x0A;192.168.10.1/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="270" top="416" right="387" bottom="448" content="vlan20&#x0D;&#x0A;192.168.20.1/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="49" top="137" right="181" bottom="169" content="G0/0/0.20:&#x0D;&#x0A;192.168.20.254/24" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="124" top="261" right="173" bottom="278" content="e0/0/1" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="238" top="261" right="295" bottom="278" content="e0/0/10" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="417" top="474" right="663" bottom="491" content="4、配置PC1、PC2 IP地址、网关地址" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
        <txttip left="415" top="511" right="646" bottom="528" content="5、测试 PC1 、PC2 之间的连通性" fontname="Consolas" fontstyle="0" editsize="100" txtcolor="-16777216" txtbkcolor="-7278960" charset="1" />
    </txttips>
</topo>
